BA-100

VIDEO IN

|  |  |
| --- | --- |
| 3G-SDI | BNC×1 |

VIDEO OUT

|  |  |
| --- | --- |
| 3G SDI | BNC×1 |
| HDMI | HDMI×1 |

AUDIO

|  |  |
| --- | --- |
| Audio demultiplexing | Support SDI embedded |

VIDEO FORMAT

|  |  |
| --- | --- |
| HDMI | Video format with SDI interface input |
| 3G-SDI | 1080p50/60 |
| HD-SDI | 1080i/60/59.94/50、1080p/30/29.97/25/24/24sF/23.98/23.98sF、720p/60/59.94/50 |
| SD-SDI | 480/59.94i、576/50i |

Operation

|  |  |
| --- | --- |
| Input voltage | 12V DC 2.0 jack plug |
| Power consumption（MAX） | ≤10W |
| Working temperature | 0-40℃ |
| Store temperature | -20-60℃ |
| Store humidity | 0%-90% No Condensation |

Structure

|  |  |
| --- | --- |
| Shell material | Aluminium-magnesium alloy |
| Dimension（mm） | 84.2（L）×108.2（D）×28.4（H）mm |
| Weight | 0.7Kg（Including Packing and spare parts ） |
| Installing way | No |
| VESA connection port | No |